|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Profile #** | **HG /HS** | **O/E or All** | **Height** | **Type** | **Shelf Type** | **Rail/Lip** | **Plexi** | **Slant** | **Base  Rail** | **Shelf Depth** | **Shelf 1 Slots** | **Shelf 2 Slots** | **Shelf 3 Slots** | **Shelf 4 Slots** | **Shelf 5 Slots** | **Shelf 6 Slots** | **Specific Notations** |
| 101 | HG | Odd | 62” | Gondola | Glass |  |  |  |  | 16” | 7/8 | 14/15 | 22/23 |  |  |  |  |
| 101 | HG | Even | 62” | Gondola | Glass |  |  |  |  | 16” | 5/6 | 12/13 | 20/21 |  |  |  |  |
| 102 | HG | Odd | 62” | Gondola | Glass |  |  |  |  | 16” | 6/7 | 11/12 | 16/17 | 21/22 |  |  |  |
| 102 | HG | Even | 62” | Gondola | Glass |  |  |  |  | 16” | 4/5 | 9/10 | 14/15 | 19/20 |  |  |  |
| 103 | HG | Odd | 62” | Gondola | Glass |  |  |  |  | 16” | 9/10 | 19/20 |  |  |  |  |  |
| 103 | HG | Even | 62” | Gondola | Glass |  |  |  |  | 16” | 8/9 | 17/18 |  |  |  |  |  |
| 104 | HG | All | 62” | Gondola | Glass |  |  |  |  | 16” | 6/7 | 14/15 | 21/22 |  |  |  |  |
| 105 | HG | All | 62” | Gondola | Glass |  |  |  |  | 16” | 4/5 | 10/11 | 16/17 | 22/23 |  |  |  |
| 106 | HG | Even | 62” | Gondola | Glass |  |  |  |  | 16” | 7/8 | 14/15 | 22/23 |  |  |  |  |
| 106 | HG | Odd | 62” | Gondola | Glass |  |  |  |  | 16” | 9/10 | 18/19 |  |  |  |  |  |
| 107 | HG | Odd | 62” | Gondola | Glass |  |  |  |  | 18” | 13/14 |  |  |  |  |  |  |
| 107 | HG | Even | 62” | Gondola | Glass |  |  |  |  | 18” | 11/12 |  |  |  |  |  |  |
| 108 | HG | All | 62” | Gondola | Metal | Rail | Yes | Yes |  | 18” | 3/4 | 8/9 | 14/15 | 20/21 | 25/26 |  | Place rail along front w/zip ties or plastic pegs and overlay the plexi-shield on each end of the rail, this profile uses slanted shelves |
| 109 | HG | Odd | 62” | Gondola | Glass | Lip |  |  |  | 16” | 6/7 | 11/12 | 17/18 | 22/23 |  |  | Place plastic lip along front edge w/rubber mallet |
| 109 | HG | Even | 62” | Gondola | Glass | Lip |  |  |  | 16” | 5/6 | 10/11 | 16/17 | 21/22 |  |  | Place plastic lip along front edge w/rubber mallet |
| 110 | HG | Odd | 62” | Gondola | Rug Arms |  |  |  |  |  | 24/25 |  |  |  |  |  | Rug arm cross bar to be placed in the correct slots with the rug arms placed into the holes on the cross bar |
| 110 | HG | All | 62” | Gondola | Metal | Rail |  | Yes |  | 22” | 8/9 | 14/15 | 20/21 | 26/27 |  |  | Place rail along front w/zip ties or plastic pegs, this profile uses slanted shelves |
| 111 | HG | All | 62” | Gondola | Glass |  |  |  |  | 16” | 6/7 | 14/15 | 21/22 |  |  |  |  |
| 112 | HG | All | 62” | Gondola | Glass |  |  |  |  | 16” | 4/5 | 10/11 | 15/16 | 20/21 |  |  |  |
| 113 | HG | Odd | 51” | Gondola | Glass |  |  |  |  | 14” | 5/6 | 11/12 | 17/18 |  |  |  |  |
| 113 | HG | Even | 51” | Gondola | Glass |  |  |  |  | 14” | 3/4 | 9/10 | 15/16 |  |  |  |  |
| 114 | HG | Odd | 62” | Gondola | Glass |  |  |  |  | 14” | 16/17 |  |  |  |  |  | Place Power Strip @ slots 3/4 and 18/19 & use 16” braces for the 14” shelves so that you have the gap in the back |
| 114 | HG | Even | 62” | Gondola | Glass |  |  |  |  | 14” | 13/14 |  |  |  |  |  | Place Power Strip @ slots 3/4 and 18/19 & use 16” braces for the 14” shelves so that you have the gap in the back |
| 115 | HG | All | 62” | Gondola | Grid |  |  |  | Yes |  |  |  |  |  |  |  | Grid panels will be needed if the Gondola it is NOT made of slatwall, you will use art brackets or j-hooks to display items and place a rail on the base deck |
| 118 | HG | Odd | 62” | Gondola | Glass |  |  |  |  | 18” | 8/9 | 17/18 |  |  |  |  |  |
| 118 | HG | Even | 62” | Gondola | Glass |  |  |  |  | 18” | 5/6 | 14/15 |  |  |  |  |  |
| 121 | HG | All | 62” | Gondola | Metal |  |  |  |  | 22” | 4/5 | 10/11 | 15/16 | 21/22 |  |  |  |
| 123 | HG | All | 62” | Gondola | Basket |  |  |  |  |  | 6/7 | 16/17 | 26/27 |  |  |  | Use large wire baskets |
| 124 | HG | Odd | 62” | Gondola | Glass & Jet Rail |  |  |  |  | 16” | 19/20 | 21/22 |  |  |  |  | Use a jet rail in shelf 1 slots and brackets for glass shelves in shelf 2 slots – you will have a glass shelf with a jet rail beneath |
| 124 | HG | Even | 62” | Gondola | Glass & Grid |  |  |  |  | 16” |  | 21/22 |  |  |  |  | Glass in shelf 2 slots with grid panels underneath |
| 201 | HG | Odd | 72” | Gondola | Glass |  |  |  |  | 16” | 7/8 | 13/14 | 20/21 | 27/28 |  |  |  |
| 201 | HG | Even | 72” | Gondola | Glass |  |  |  |  | 16” | 4/5 | 11/12 | 18/19 | 25/26 |  |  |  |
| 202 | HG | Odd | 72” | Gondola | Glass |  |  |  |  | 18” | 9/10 | 20/21 |  |  |  |  |  |
| 202 | HG | Even | 72” | Gondola | Glass |  |  |  |  | 18” | 7/8 | 18/19 |  |  |  |  |  |
| 203 | HG | Odd | 72” | Gondola | Glass |  |  |  |  | 18” | 9/10 | 17/18 | 25/26 |  |  |  |  |
| 203 | HG | Even | 72” | Gondola | Glass |  |  |  |  | 18” | 8/9 | 16/17 | 24/25 |  |  |  |  |
| 204 | HG | All | 72” | Gondola | Metal |  |  |  |  | 20” | 11/12 | 18/19 |  |  |  |  |  |
| 205 | HG | All | 72” | Gondola | Metal |  |  |  |  | 20” | 9/10 | 20/21 |  |  |  |  |  |
| 206 | HG | All | 72” | Gondola | Metal | Rail |  |  |  | 20” | 7/8 | 15/16 | 23/24 |  |  |  | Place rail along front w/zip ties or plastic pegs |
| 207 | HG | All | 72” | Gondola | Metal | Rail |  |  | Yes | 20” | 7/8 | 16/17 | 25/26 |  |  |  | Place rail along front w/zip ties or plastic pegs and place a rail on the base deck |
| 208 | HG | Odd | 72” | Gondola | Glass |  |  |  |  | 14” | 20/21 |  |  |  |  |  | Place Power Strip @ slots 3/4 and 18/19 & use 16” braces for the 14” shelves so that you have the gap in the back |
| 208 | HG | Even | 72” | Gondola | Glass |  |  |  |  | 14” | 16/17 |  |  |  |  |  | Place Power Strip @ slots 3/4 and 18/19 & use 16” braces for the 14” shelves so that you have the gap in the back |
| 209 | HG | All | 72” | Gondola | Glass |  |  |  |  | 14” | 7/8 | 15/16 | 23/24 |  |  |  | Place Power Strip @ slots 3/4 and 18/19 & use 16” braces for the 14” shelves so that you have the gap in the back |
| 210 | HG | All | 72” | Gondola | Grid |  |  |  | Yes |  |  |  |  |  |  |  | place a rail on the base deck |
| 211 | HG | Odd | 72” | Gondola | Rug Arms |  |  |  |  |  | 16/17 | 31/32 |  |  |  |  |  |
| 211 | HG | Even | 72” | Gondola | Metal | Rail |  | Yes |  | 22” | 8/9 | 14/15 | 19/20 | 25/26 | 31/32 |  | Metal shelf with rail around the edge, this profile uses slanted shelves |
| 213 | HG | All | 72” | Gondola | Glass |  |  |  |  | 16” | 8/9 | 17/18 | 26/27 |  |  |  |  |
| 214 | HG | Odd | 72” | Gondola | Glass |  |  |  |  | 16” | 6/7 | 11/12 | 16/17 | 21/22 | 26/27 |  |  |
| 214 | HG | Even | 72” | Gondola | Glass |  |  |  |  | 16” | 4/5 | 9/10 | 14/15 | 19/20 | 24/25 |  |  |
| 215 | HG | All | 72” | Gondola | Glass |  |  |  |  | 16” | 4/5 | 9/10 | 15/16 | 20/21 | 26/27 |  |  |
| 216 | HG | All | 72” | Gondola | Metal | Rail | Yes | Yes |  | 18” | 3/4 | 8/9 | 13/14 | 18/19 | 23/24 | 28/29 | Place rail along front w/zip ties or plastic pegs and overlay the plexi-shield on each end of the rail, this profile uses slanted shelves |
| 217 | HG | Odd | 72” | Gondola | Glass |  |  |  |  | 16” | 7/8 | 15/16 | 23/24 |  |  |  |  |
| 217 | HG | Even | 72” | Gondola | Glass |  |  |  |  | 16” | 5/6 | 13/14 | 21/22 |  |  |  |  |
| 218 | HG | Odd | 72” | Gondola | Glass | Lip |  |  |  | 16” | 8/9 | 15/16 | 21/22 | 27/28 |  |  | Place plastic lip along front edge w/rubber mallet |
| 218 | HG | Even | 72” | Gondola | Glass | Lip |  |  |  | 16” | 7/8 | 14/15 | 20/21 | 26/27 |  |  | Place plastic lip along front edge w/rubber mallet |
| 219 | HG | All | 72” | Gondola | Metal | Rail |  |  | Yes | 14” | 9/10 | 17/18 | 24/25 |  |  |  | Place rail along front w/zip ties or plastic pegs and place a rail on the base deck |
| 220 | HG | All | 72” | Gondola | Metal | Rail |  |  | Yes | 20” | 9/10 | 18/19 | 27/28 |  |  |  | Place rail along front w/zip ties or plastic pegs and place a rail on the base deck |
| 221 | HG | All | 72” | Gondola | Metal |  |  |  |  | 22” | 4/5 | 10/11 | 15/16 | 21/22 | 26/27 |  |  |
| 222 | HG | Even | 72” | Gondola | Glass |  |  |  |  | 16” | 7/8 | 14/15 | 21/22 | 27/28 |  |  |  |
| 223 | HG | All | 72” | Gondola | Basket |  |  |  |  |  | 6/7 | 16/17 | 26/27 |  |  |  | Use large wire baskets |
| 224 | HG | Odd | 72” | Gondola | Glass |  |  |  |  | 16” | 24/25 | 26/27 |  |  |  |  | Use a jet rail in shelf 1 slots and brackets for glass shelves in shelf 2 slots – you will have a glass shelf with a jet rail beneath |
| 224 | HG | Even | 72” | Gondola | Glass |  |  |  |  | 16” |  | 26/27 |  |  |  |  | Use a jet rail in shelf 1 slots and brackets for glass shelves in shelf 2 slots – you will have a glass shelf with a jet rail beneath |
| 301 | HG | Odd |  | Wall | Glass |  |  |  |  | 16” | 8/9 | 15/16 | 23/24 | 30/31 |  |  |  |
| 301 | HG | Even |  | Wall | Glass |  |  |  |  | 16” | 5/6 | 13/14 | 20/21 | 28/29 |  |  |  |
| 302 | HG | Odd |  | Wall | Glass |  |  |  |  | 16” | 7/8 | 13/14 | 19/20 | 25/26 | 30/31 |  |  |
| 302 | HG | Even |  | Wall | Glass |  |  |  |  | 16” | 5/6 | 11/12 | 17/18 | 23/24 | 28/29 |  |  |
| 304 | HG | All |  | Wall | Glass |  |  |  |  | 18” | 7/8 | 15/16 | 23/24 | 31/32 |  |  |  |
| 306 | HG | Odd |  | Wall | Glass |  |  |  |  | 18” | 13/14 | 26/27 |  |  |  |  |  |
| 306 | HG | Even |  | Wall | Glass |  |  |  |  | 18” | 10/11 | 23/24 |  |  |  |  |  |
| 307 | HG | Odd |  | Wall | Glass |  |  |  |  | 18” | 10/11 | 20/21 | 30/31 |  |  |  |  |
| 307 | HG | Even |  | Wall | Glass |  |  |  |  | 18” | 7/8 | 17/18 | 27/28 |  |  |  |  |
| 308 | HG | All |  | Wall | Metal |  |  |  |  | 20” | 10/11 | 20/21 | 30/31 |  |  |  |  |
| 309 |  | All |  | Wall | Glass |  |  |  |  | 16” & 18” | 4/5 | 9/10 | 15/16 | 21/22 | 27/28 | 33/34 | 2 sizes of shelves being used:  18” in shelf slots 1 & 2 16” in shelf slots 3 - 6 |
| 310 | HG | All |  | Wall | Metal |  |  |  |  | 20” | 7/8 | 15/16 | 22/23 | 30/31 |  |  |  |
| 311 | HG | Odd |  | Wall | Rug Arms |  |  |  |  |  | 14/15 | 29/30 |  |  |  |  |  |
| 311 | HG | Even |  | Wall | Metal | Rail |  | Yes |  | 22” | 6/7 | 12/13 | 17/18 | 23/24 | 29/30 |  | Place rail along front w/zip ties or plastic pegs, this profile uses slanted shelves |
| 313 | HG | Odd |  | Wall | Glass |  |  |  |  | 14” | 18/19 |  |  |  |  |  | Place Power Strip @ slots 4/5 and 16/17 & use 16” braces for the 14” shelves so that you have the gap in the back |
| 313 | HG | Even |  | Wall | Glass |  |  |  |  | 14” | 16/17 |  |  |  |  |  | Place Power Strip @ slots 4/5 and 16/17 & use 16” braces for the 14” shelves so that you have the gap in the back |
| 314 | HG | All |  | Wall | Grid |  |  |  | Yes |  |  |  |  |  |  |  | You will use art brackets or  j-hooks to display items and place a rail on the base deck |
| 319 | HG | All |  | Wall | Metal | Rail |  |  | Yes | 14”& 18” | 7/8 | 15/16 | 22/23 |  |  |  | 2 sizes of shelves being used:  18” in shelf slots 1 & 2 14” in shelf slot 3  Place rail along front w/zip ties or plastic pegs and place a rail on the base deck |
| 321 | HG | All |  | Wall | Metal |  |  |  | Yes | 22” | 4/5 | 10/11 | 15/16 | 21/22 | 26/27 |  | Place a rail on the base deck |
| 323 | HG | All |  | Wall | Basket |  |  |  |  |  | 6/7 | 16/17 | 26/27 |  |  |  | Use large baskets |
| 324 | HG | Odd |  | Wall | Glass & Jet Rail |  |  |  |  | 16” | 17/18 | 29/30 | 31/32 |  |  |  | Use a jet rail in shelf 1 slots and brackets for glass shelves in shelf 2 slots – you will have a glass shelf with a jet rail beneath |
| 324 | HG | Even |  | Wall | Glass & Grids |  |  |  |  | 16” |  |  | 31/32 |  |  |  | Glass shelf above with use grid panels under the glass in shelf 3 slots |
| 401 | HG | All | 62” | Endcap | Glass |  |  |  |  | 16” | 6/7 | 13/14 | 20/21 |  |  |  |  |
| 402 | HG | All | 62” | Endcap | Glass |  |  |  |  | 16” | 4/5 | 10/11 | 15/16 | 21/22 |  |  |  |
| 403 | HG | All | 62” | Endcap | Metal | Rail | Yes | Yes |  | 18” | 3/4 | 8/9 | 14/15 | 19/20 | 23/24 |  | Place rail along front w/zip ties or plastic pegs and overlay the plexi-shield on each end of the rail, this profile uses slanted shelves |
| 404 | HG | All | 62” | Endcap | Glass |  |  |  |  | 16” | 7/8 | 16/17 |  |  |  |  |  |
| 405 | HG | All | 72” | Endcap | Glass |  |  |  |  | 16” | 7/8 | 15/16 | 23/24 |  |  |  |  |
| 406 | HG | All | 72” | Endcap | Metal |  |  |  |  | 16” | 6/7 | 13/14 | 20/21 |  |  |  |  |
| 407 | HG | All | 72” | Endcap | Metal |  |  |  |  | 16” | 7/8 | 15/16 | 23/24 |  |  |  |  |
| 408 | HG | All | 72” | Endcap | Glass |  |  |  |  | 14” | 16/17 |  |  |  |  |  | Place Power Strip @ slots 1/2 and 18/19 & use 16” braces for the 14” shelves so that you have the gap in the back |
| 409 | HG | All | 62” | Endcap | Grid |  |  |  | Yes |  |  |  |  |  |  |  | Grids will be needed if Gondola it is NOT made of slatwall, you will use art brackets or j-hooks and place a rail on the base deck |
| 411 | HG | All | 72” | Endcap | Glass |  |  |  |  | 16” | 6/7 | 13/14 | 20/21 | 27/28 |  |  |  |
| 413 | HG | All | 62” | Endcap | Metal |  |  |  |  | 16” | 4/5 | 10/11 | 15/16 | 23/22 |  |  |  |
| 414 | HG | All | 72” | Endcap | Metal |  |  |  |  | 16” | 4/5 | 10/11 | 15/16 | 21/22 | 26/27 |  |  |
| 415 | HG | All | 72” | Endcap | Glass |  |  |  |  | 16” | 4/5 | 10/11 | 15/16 | 21/22 | 26/27 |  |  |
| 416 | HG | All | 72” | Endcap | Metal | Rail | Yes | Yes |  | 18” | 3/4 | 8/9 | 13/14 | 18/19 | 23/24 | 28/29 | Place rail along front w/zip ties or plastic pegs and overlay the plexi-shield on each end of the rail, this profile uses slanted shelves |
| 419 | HG | All | 72” | Endcap | Metal | Rail |  |  | Yes | 14” & 18” | 7/8 | 15/16 | 23/24 |  |  |  | 2 sizes of shelving used:  18” in shelf slots number 1 & 2 14” in shelf slot number 3  these shelves should have the metal rail on a 3 sides and you’ll need to place a rail on the base deck |
| 501 | HG | Odd |  | Focal Wall | Glass |  |  |  |  | 16” | 8/9 | 15/16 | 23/24 | 30/31 |  |  | 16” glass within faux wood frame |
| 501 | HG | Even |  | Focal Wall | Glass |  |  |  |  | 16” | 5/6 | 13/14 | 20/21 | 28/29 |  |  | 16” glass within faux wood frame |
| 506 | HG | Odd |  | Focal Wall | Glass |  |  |  |  | 18” | 13/14 | 26/27 |  |  |  |  | 18” glass within faux wood frame |
| 506 | HG | Even |  | Focal Wall | Glass |  |  |  |  | 18” | 10/11 | 23/24 |  |  |  |  | 18” glass within faux wood frame |
| 507 | HG | Odd |  | Focal Wall | Glass |  |  |  |  | 18” | 10/11 | 20/21 | 30/31 |  |  |  | 18” glass within faux wood frame |
| 507 | HG | Even |  | Focal Wall | Glass |  |  |  |  | 18” | 7/8 | 17/18 | 27/28 |  |  |  | 18” glass within faux wood frame |
| 508 | HG | All |  | Focal Wall | Glass |  |  |  |  | 20” | 10/11 | 20/21 | 31/31 |  |  |  | 20” glass within faux wood frame |
| 514 | HG | All |  | Focal Wall | Grid |  |  |  | Yes |  |  |  |  |  |  |  | You will use art brackets or j-hooks to display items and place a rail on the base deck |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 101 | HS | Odd | 62” | Workhorse | Glass |  |  |  |  | 16” |  |  |  |  |  |  | No slot numbers given, just 2 shelves shown |
| 101 | HS | Even | 62” | Workhorse | Grid |  |  |  |  |  |  |  |  |  |  |  | Full coverage grid panels |
| 102 | HS | All | 62” | Endcap | Glass |  |  |  |  | 16” |  |  |  |  |  |  | No slot numbers given, just 3 shelves shown |
| 201 | HS | Odd | 72” | Workhorse | Rug Arm |  |  |  |  |  |  |  |  |  |  |  | SCATTER RUG / no slot numbers given, just 2 rug arms shown in place |
| 201 | HS | Even | 72” | Workhorse | Metal |  |  |  |  | 22” |  |  |  |  |  |  | SCATTER RUG / no slot numbers given, just four 22” bullnose shelves shown |
| 202 | HS |  | 72” | Endcap | Metal |  |  |  |  | 22” |  |  |  |  |  |  | SCATTER RUG / no slot numbers given, just four 22” bullnose shelves shown |
| 204 | HS |  | 72” | Endcap | Metal |  |  |  |  | 22” |  |  |  |  |  |  | ACCENT FURNITURE / no slot numbers given, just two 22” bullnose shelves shown |
| 301 | HS |  | 84” | Endcap | Glass |  |  |  |  | 16” | 6/7 | 13/14 | 20/21 | 27/28 |  |  | NO Department Identifiers |
| 302 | HS |  | 84” | Endcap | Glass |  |  |  |  | 16” | 4/5 | 11/12 | 19/20 | 27/28 |  |  | BOOKS (D33) / GIFTS |
| 303 | HS | Odd | 84” |  | Grid & Glass |  |  |  |  | 16” | 6/7 | 14/15 | 17/23 | 24/30 | 31/36 |  | PARTY / Glass shelves go into slots 1 & 2 and then grid panels go above the shelves |
| 303 | HS | Even | 84” |  | Grid |  |  |  |  |  |  |  |  |  |  |  | PARTY / Full coverage grid panels |
| 304 | HS | Odd | 84” | Workhorse | Glass |  |  |  |  | 16” | 8/9 | 17/18 | 26/27 |  |  |  | STATIONARY / Acrylic Bookcases can be used |
| 304 | HS | Even | 84” | Workhorse | Glass |  |  |  |  | 16” | 7/8 | 14/15 | 21/22 | 28/29 |  |  | STATIONARY |
| 305 | HS |  | 84” | Workhorse | Glass |  |  |  |  | 16” | 5/6 | 12/13 | 18/19 | 23/24 | 29/30 |  | SPA / FRAMES has SPA typed below it and had FRAMES written below it, assuming its for both |
| 306 | HS | Odd | 84” | Workhorse | Grid |  |  |  |  |  |  |  |  |  |  |  | COLLAGES / Full coverage grid panels |
| 306 | HS | Even | 84” | Workhorse | Grid |  |  |  |  |  |  |  |  |  |  |  | COLLAGES / Full coverage grid panels with notation to use art brackets ONLY within 306 EVEN |
| 307 | HS | Odd | 84” | Workhorse | Glass |  |  |  |  | 16” | 4/5 | 10/11 | 16/17 | 22/23 | 28/29 |  | CANDLES |
| 307 | HS | Even | 84” | Workhorse | Glass |  |  |  |  | 16” | 3/4 | 8/9 | 14/15 | 20/21 | 26/27 |  | CANDLES |
| 308 | HS | Odd | 84” | Workhorse | Glass |  |  |  |  | 16” | 8/9 | 17/18 | 25/26 |  |  |  | FLEX |
| 308 | HS | Even | 84” | Workhorse | Glass |  |  |  |  | 16” | 5/6 | 11/12 | 22/23 |  |  |  | FLEX |
| 310 | HS | Odd | 84” | Workhorse | Glass |  |  |  |  | 16” | 9/10 | 19/20 | 29/30 |  |  |  | DESIGN ACCENTS |
| 310 | HS | Even | 84” | Workhorse | Glass |  |  |  |  | 16” | 8/9 | 18/19 | 27/28 |  |  |  | DESIGN ACCENTS |
| 311 | HS | Odd | 84” | Workhorse | Hang Bar |  |  |  |  | 12” | 16/17 | 34/35 |  |  |  |  | WINDOW / 2 - Hang Bars |
| 311 | HS | Even | 84” | Workhorse | Glass |  |  |  |  | 15” | 15/16 | 33/34 |  |  |  |  | WINDOW / Cross Bar with 15” face-out hooks |
| 312 | HS | All | 84” | Workhorse | Glass |  |  |  |  | 16” | 7/8 | 15/16 | 24/25 | 32/33 |  |  | DEC PILLOWS / Really???  Pillows are usually on the wall, if this is the horse then the shelf spacings seems really off!!!, even in the picture it looks horrible |
| 313 | HS | Odd | 84” | Workhorse | Glass |  |  |  |  | 16” | 21/22 | 23/24 | 29/30 |  |  |  | THROWS / Use a Cross Bar in shelf 1 slots and brackets for glass shelves in shelf 2 & shelf 3 slots – you will have a 2 glass shelves with a cross bar beneath with face out hooks placed on the bar |
| 313 | HS | Even | 84” | Workhorse | Glass |  |  |  |  | 16” | 23/24 | 24/25 | 30/31 |  |  |  | THROWS / Use a Hang Bar in shelf 1 slots and brackets for glass shelves in shelf 2 & shelf 3 slots – you will have a 2 glass shelves with a 12” hang bar beneath |
| 314 | HS |  | 84” | EndCap | Glass |  |  |  |  | 16” | 21/22 | 23/24 | 29/30 |  |  |  | THROWS / Use a Cross Bar in shelf 1 slots and brackets for glass shelves in shelf 2 & shelf 3 slots – you will have a 2 glass shelves with a cross bar beneath with 2-3 face out hooks placed on the bar |
| 321 | HS | Odd | 84” | Workhorse | Glass |  |  |  |  | 18” | 12/13 | 23/24 |  |  |  |  | ORGANIZE / LAUNDRY |
| 321 | HS | Even | 84” | Workhorse | Grid |  |  |  |  |  |  |  |  |  |  |  | ORGANIZE / LAUNDRY - Full coverage grid panels |
| 322 | HS | Odd | 84” | Workhorse | Hang Bar |  |  |  |  | 12” | 7/8 | 13/14 | 19/20 | 26/26 | 31/32 |  | CLOSET / HANGERS - 12” Hang bars in all slots |
| 322 | HS | Even | 84” | Workhorse | Glass |  |  |  |  | 18” | 11/12 | 19/20 | 30/31 |  |  |  | CLOSET |
| 330 | HS | Odd | 84” | Workhorse | Grid |  |  |  |  |  |  |  |  |  |  |  | UTILITY / HARDWARE - Full coverage grid panels |
| 330 | HS | Even | 84” | Workhorse | Glass |  |  |  |  | 18” | 7/8 | 17/18 | 27/28 | 30/31 |  |  | UTILITY / HARDWARE |
| 331 | HS | Odd | 84” | Workhorse | Grid |  |  |  |  |  |  |  |  |  |  |  | UTILITY / BATH - Full coverage grid panels |
| 331 | HS | Even | 84” | Workhorse | Glass |  |  |  |  | 16” | 8/9 | 13/14 | 18/19 | 25/26 |  |  | UTILITY / BATH |
| 332 | HS | All | 84” | Workhorse | Grid & Glass |  |  |  |  | 18” | 6/7 | 10/11 | 14/15 | 18/19 |  |  | CLEAN - (For 1st section only!) Glass shelves go into slots 1 - 4 and then the 2 grid panels go above those shelves, additional sections will fall under profile #337. |
| 336 | HS | Odd | 84” | Workhorse | Glass |  |  |  |  | 16” | 3/4 | 11/12 | 19/20 | 27/28 |  |  | DEC KITCHEN / BAR / KITCHEN ACCESSORIES |
| 336 | HS | Even | 84” | Workhorse | Glass |  |  |  |  | 16” | 5/6 | 12/13 | 20/21 | 28/29 |  |  | DEC KITCHEN / BAR / KITCHEN ACCESSORIES |
| 337 | HS | All | 84” | Workhorse | Grid |  |  |  |  |  |  |  |  |  |  |  | FRY / GADGETS / KITCHEN TEXTILES / CLEAN - Full coverage grid panels |
| 338 | HS | Odd | 84” | Workhorse | Glass |  |  |  |  | 16” | 3/4 | 9/10 | 16/17 | 21/22 | 28/29 |  | PANTRY |
| 338 | HS | Even | 84” | Workhorse | Glass |  |  |  |  | 16” | 2/3 | 8/9 | 15/16 | 20/21 | 27/28 |  | PANTRY |
| 339 | HS |  | 84” | Workhorse | Glass | Yes\* |  | Yes |  | 16” | 4/5 | 11/12 | 25/26\* | 35/36\* |  |  | LINEN - Shelves into slots 1 & 2 should be placed flat (without a slant) shelves in slots 3 & 4 should be slanted downward, a sheet rail will be inserted on the front edge of the 2 slanted shelves. |
| 340 | HS |  | 84” | Workhorse | Glass |  |  |  |  | 18” | 15/16 | 30/31 |  |  |  |  | RECYCLE |
| 341 | HS | Odd | 84” | Workhorse | Glass |  |  |  |  | 18” | 13/14 | 20/21 | 28/29 |  |  |  | WORK @ HOME |
| 341 | HS | Even | 84” | Workhorse | Glass |  |  |  |  | 18” | 14/15 | 22/23 | 29/30 |  |  |  | WORK @ HOME |
| 342 | HS | Odd | 84” | Workhorse | Grid |  |  |  |  |  |  |  |  |  |  |  | WORK @ HOME - Full coverage grid panels |
| 342 | HS | Even | 84” | Workhorse | Glass |  |  |  |  | 18” | 14/15 | 22/23 | 29/30 |  |  |  | WORK @ HOME. - |
| 343 | HS | All | 84” | Workhorse | Glass |  |  |  |  | 16” | 2/3 | 9/10 | 15/16 | 20/21 | 26/27 |  | BAKE CAFE |
| 345 | HS | All | 84” | Workhorse | Glass | Yes |  |  |  | 16” | 15/16 | 30/31 |  |  |  |  | BEDDING - a sheet rail will be inserted on the front edge of these 2 shelves. |